Crankshaft Balancer Removal. Cadillac Concours 1996

For 1990-2009 cars

#### Tools Required

• | J 38416-2 Crankshaft Button

• | J 41816 Crankshaft Balancer Remover

• | J 44214 Flywheel Holder

1. Install the J 44214 to the engine block.
2. Secure the flywheel in order to prevent crankshaft rotation.
3. Remove the crankshaft balancer bolt.
4. Place the J 38416-2 in the end of the crankshaft.
5. Position the legs of the J 41816 onto the backside of the balancer inner hub.
6. Tighten the center screw on the puller until the balancer pulls clear of the crankshaft end.
7. Remove the crankshaft balancer.