Lower Control Valve Body Assembly Removal. Cadillac Concours 1997

For 1990-2009 cars

1. Use a small screwdriver in order to disconnect the manual valve linkage clip (915).
2. Use a small screwdriver in order to disconnect the electrical connectors from the following parts:

• | The 1-2 shift solenoid valve (909)

• | The 2-3 shift solenoid valve (909)

• | The automatic transmission fluid pressure manual valve position switch (936)

3. Remove the wire harness from the two wiring harness clips.
4. Remove the nine 10 mm bolts (534) from the oil transfer plate (956).
5. Remove the oil transfer plate (956).
6. Remove the two 10 mm nuts and the eleven 10 mm bolts from the lower controls assembly. Do not remove the four bolts indicated.
7. Lift the lower channel plate, control valve body and accumulator assembly from the case as a single unit.