Pump Installation. Cadillac Concours 1997

For 1990-2009 cars

#### Tools Required

J 39068 Pump Assembly Guide Pins

1. Install the J 39068 into the case.
2. Install the new gasket (228).
3. Install the pump assembly (200-225).
4. Apply pipe thread sealant, GM P/N 12346004 to pump bolt threads before installation.
5. Hand start all of the bolts (229, 231, 232, 233, 234, 235, 331).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

6. Remove the guide pins and install the remaining bolts.

Tighten
Tighten the bolts in sequence in a clockwise pattern to 11-13 N·m (8.0-9.5 lb ft).