Water Crossover Removal. Cadillac Concours 1997

For 1990-2009 cars

1. Remove the lift bracket retaining studs (2).
2. Remove the lift bracket (1) from the cylinder head.
3. Remove the coolant temperature sensor from the cylinder head.
4. Remove the EGR valve bolts.
5. Remove the EGR valve and the gasket.
6. Loosen the water crossover mounting bolts (1-5).
7. Remove the water crossover and all mounting bolts (1-3).
8. Remove the upper (1) and lower (2) water crossover gaskets. Do not damage the water crossover gaskets. These gaskets are reusable.