Shift Cable Replacement. Cadillac Concours 1997

For 1990-2009 cars

### Removal Procedure

1. Remove the cable end cap from the transmission park/neutral position switch lever.
2. Remove the cable from the bracket by prying on the lock button to the unlocked position.
3. Remove the left I/P sound insulator. Refer to Sound Insulators in Instrument Panel, Gauges and Console.
4. Remove the console center trim panel. Refer to Shifter Trim Plate in Instrument Panel, Gauges, and Console.
5. Remove the shift control cable from the floor shift assembly.
6. Remove the cable from the vehicle.

### Installation Procedure

1. Install the shift control cable to the vehicle.
2. Install the cable end cap to the floor shift assembly.
3. Install the console center trim panel. Refer to Shifter Trim Plate in Instrument Panel, Gauges and Console.
4. Install the left I/P sound insulator. Refer to Sound Insulators in Instrument Panel, Gauges and Console.
5. Install the cable into the retaining bracket. Push down on the locking tab. Refer to Range Selector Lever Cable Adjustment .
6. Install the cable end cap to the transmission position switch lever.