DTC P1814 Torque Converter Overstressed. Cadillac Concours 1996

For 1990-2009 cars
Automatic Transmission Components
Automatic Transmission Controls Schematics
OBD II Symbol Description Notice

### Circuit Description

This diagnostic test checks for unusually high throttle angle and low vehicle speed when the transmission is in Drive or Reverse. The primary purpose of this DTC is to record the Failure Record data, because this condition could damage the Powertrain or create an unsafe condition. This is a Type D DTC.

### Conditions for Setting the DTC

• | No TP DTCs P0121, P0122, or P0123 are set.

• | No VSS DTCs P0502 or P0503 are set.

• | No A/T ISS DTCs P0716 or P0717 are set.

• | The slip is greater than 1600 RPM.

• | The vehicle speed is less than 8 km/h (5 mph).

• | The transmission is in Drive or Reverse.

• | The throttle angle is 75° or greater for 12 seconds.

### Action Taken When the DTC Sets

DTC P1814 is recorded in history.

### Conditions for Clearing the DTC

A scan tool can clear the DTC from the PCM history. The PCM clears the DTC from the PCM history if the vehicle completes 40 warm-up cycles without a failure reported.

### Diagnostic Aids

A simultaneous acceleration and application of the brakes may cause the DTC to set.

### Test Description

The numbers below refer to the step numbers on the diagnostic chart.

1. This Step verifies that the Powertrain On-Board Diagnostic System Check was performed.

2. This Step inspects the failure records for DTC P1814 occurrences.

3. This Step inspects the fluid level and color. If the fluid level and color are suspect, refer to Transmission Fluid Check .

4. Important: Reset the Trans Oil Life when you replace the fluid and the filter.

   This Step replaces the fluid and the filter. If DTC P1814 occurs more than once in the failure records, severe TCC damage may have occurred.

#### DTC P1814 Torque Converter Overstress

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Powertrain On-Board Diagnostic (OBD) System Check performed? | -- | Go to Step 2 | Go to A Powertrain On Board Diagnostic (OBD) System Check

2

1. Install the scan tool (tech 1) .
2. With the engine OFF, turn the ignition switch to the RUN position.

Important: Before clearing the DTCs, use the scan tool in order to record the Failure Records for reference. The Clear Info function will erase the data.

3. Record the DTC Failure Records.

Does DTC P1814 failure counter indicate more than 1?

--

Go to Step 4

Go to Step 3

3 | Inspect the transmission fluid level and color. Refer to Transmission Fluid Check . Is the inspection complete? | -- | Go to Step 5 | --

4

1. Replace the transmission fluid and the scavenge screens.

Important: Reset the Trans Oil Life when you replace the fluid and the filter.

Is the repair complete?

--

Go to Step 5

--

5

In order to verify your repair, perform the following procedure:

1. Select DTC.
2. Select Clear Info.
3. Operate the vehicle under the following conditions:

• | Road test the vehicle with the gear select lever in D4.

- | The TCC slip must be less than 1504 RPM.

- | The TP Angle must be less than 65°.

- | The vehicle speed must be greater than 8 km/h (5 mph).

• | These conditions must occur for more than 5 seconds.

4. Select Specific DTC. Enter DTC P1814.

Has the test run and passed?

--

System OK

Begin the diagnosis again. Go to Step 1