Valve Removal. Cadillac Concours 1996

For 1990-2009 cars

#### Tools Required

• | J 8062 Valve Spring Compressor

• | J 38821 Valve Spring Compressor Adapter

• | J 38819 Valve Keeper Installer

• | J 38820 Valve Stem Seal Installer

1. Using an appropriately sized deep socket and a plastic hammer, lightly tap on the valve spring retainer in order to loosen the valve keepers.
2. Compress the valve spring with the J 8062 and the J 38821 .
3. Use the magnetic end of the J 38819 in order to remove the valve keepers.
4. Remove the valve spring compressor and the pilot.
5. Remove the valve spring.
6. Remove the valve seal. Use the J 38820 .
7. Remove the valve.
8. Repeat the procedure for the remaining valves.