HIGH EFFORT REQUIRED TO LIFT REAR COMPARTMENT. Cadillac Concours 1995

For 1990-2009 cars

# HIGH EFFORT REQUIRED TO LIFT REAR COMPARTMENT

#### SUBJECT: HIGH EFFORT REQUIRED TO LIFT REAR COMPARTMENT LID (ADJUST/MODIFY EXISTING TORQUE RODS)

#### MODELS: 1995 CADILLAC CONCOURS, DEVILLE

#### CONDITION:

SOME OWNERS MAY COMMENT ON THE HIGH EFFORT REQUIRED TO LIFT THE REAR COMPARTMENT LID.

#### CAUSE:

LATE DESIGN CHANGES MOVED THE TORQUE RODS FROM THE INBOARD SIDE OF THE HINGE ASSEMBLY TO THE OUTBOARD SIDE OF THE HINGE ASSEMBLY. THE CHANGE IN DESIGN INTRODUCES AN INTERFERENCE OF THE TORQUE ROD WITH THE REAR SHELF PANEL.

#### CORRECTION:

SOME VEHICLES MAY REQUIRE INCREASED TORQUE TO LIFT THE REAR COMPARTMENT LID. IN SOME CASES CASES, THIS WILL REQUIRE THE TORQUE ROD BE PLACED IN THE UPPERMOST "NOTCH" ON THE HINGE ASSEMBLY. HOWEVER, IN MOST CASES, THE TORQUE ROD CANNOT BE ADJUSTED TO THE UPPER NOTCH DUE TO AN INTERFERENCE WITH THE REAR SHELF PANEL.

USE NEW TORQUE ROD ADJUSTMENT TOOL, J-41358-1A, AND MODIFY TORQUE RODS IF NECESSARY. THE TORQUE ROD ADJUSTMENT TOOL (J-39384-1) CALLED OUT IN SECTION 10-8 OF THE SERVICE MANUAL CAN NO LONGER BE USED SINCE IT WILL ALSO INTERFERE WITH THE REAR SHELF PANEL.

1. POSITION TORQUE ROD ADJUSTMENT TOOL, J-41358-1A, TO THE OUTBOARD SIDE OF TORQUE ROD (SEE FIGURE 1). ATTEMPT TO ADJUST TORQUE RODS. IF TORQUE ROD COMES IN CONTACT WITH THE REAR SHELF PANEL, IT WILL BE NECESSARY TO MODIFY THE TORQUE ROD.

2. USING A SUITABLE TOOL, REMOVE APPROXIMATELY 16MM (5/8") OF MATERIAL FROM THE END OF THE TORQUE ROD TO ELIMINATE THE INTERFERENCE (SEE FIGURE 2).

3. ADJUST TORQUE RODS USING TORQUE ADJUSTMENT TOOL, J-41358-1A.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: B5463 (RIGHT) B5464 (LEFT) LABOR TIME: 0.2 HR (TO ADJUST TORQUE RODS) ADD: 0.1 HR (TO MODIFY TORQUE RODS, WHEN REQUIRED)

FIGURES: 2 ATTACHMENTS: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.