Oil Filter Adapter Installation. Cadillac Concours 1997

For 1990-2009 cars

1. Position the oil filter adapter on the crankcase.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the oil filter adapter bolts.

Tighten
Tighten the oil filter adapter bolts to 16 N·m (12 lb ft).

3. Install the oil pressure sensor.

Tighten
Tighten the oil pressure sensor to 16 N·m (12 lb ft).

4. Fill the oil filter with oil.
5. Install the oil filter.

Tighten
Tighten the oil filter to 32 N·m (24 lb ft).

6. Install the generator/air conditioning compressor mounting bracket.
7. Install the generator/air conditioning compressor mounting bracket bolts.

Tighten
Tighten the generator/air conditioning compressor mounting bracket bolts to 50 N·m (37 lb ft).