SMU - SEC. 6 - REV. SETTING CAMSHAFT TIMING PROC.. Cadillac Concours 1996

For 1990-2009 cars

# SMU - SEC. 6 - REV. SETTING CAMSHAFT TIMING PROC.

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 6 - REVISED SETTING CAMSHAFT TIMING PROCEDURE FOR ON VEHICLE SERVICE

#### MODELS: 1996-97 CADILLAC DEVILLE, ELDORADO, SEVILLE 1996-97 OLDSMOBILE AURORA WITH 4.0L OR 4.6L ENGINE (VINS C, Y, 9 - RPOS L47, LD8, L37)

THIS BULLETIN IS BEING ISSUED TO REVISE THE SETTING CAMSHAFT TIMING PROCEDURE IN SECTION 6 - ENGINE MECHANICAL - REPAIR INSTRUCTIONS OF THE SERVICE MANUAL.

PROCEDURE

SETTING CAMSHAFT TIMING

SETTING THE CAMSHAFT TIMING IS NECESSARY WHENEVER THE CAMSHAFT DRIVE SYSTEM HAS BEEN DISTURBED, SUCH THAT THE RELATIONSHIP BETWEEN ANY CHAIN AND SPROCKET HAS BEEN LOST. EVEN WHEN ONLY ONE SPROCKET IS INVOLVED, THE FOLLOWING PROCEDURE SHOULD BE OBSERVED SINCE ONE CRANKSHAFT ROTATION WILL NOT PROVIDE CONDITIONS WHERE CORRECT TIMING CAN BE CONFIRMED.

THE CAMSHAFTS AND CRANKSHAFT EVENTS ARE CORRECTLY TIMED WHEN THE RELATIONSHIPS SHOWN EXIST. THE FOLLOWING PROCEDURE EXPLAINS HOW TO ESTABLISH THIS CONDITION. CORRECT TIMING EXISTS WHEN THE CRANK SPROCKET AND THE INTERMEDIATE SHAFT SPROCKET HAVE THEIR TIMING MARKS ALIGNED AND ALL FOUR CAMSHAFT DRIVE PINS ARE PERPENDICULAR (90 DEGREES) TO THE CYLINDER HEAD SURFACE.

#### TOOLS REQUIRED:

- J 39946 CRANKSHAFT ROTATION SOCKET

- J 39411 FLYWHEEL HOLDER

1. REMOVE THE FOLLOWING COMPONENTS FOR ACCESS:

O THE LEFT CAMSHAFT COVER. REFER TO VALVE ROCKER ARM COVER REPLACEMENT (LEFT).

O THE RIGHT CAMSHAFT COVER. REFER TO VALVE ROCKER ARM COVER REPLACEMENT (RIGHT).

O THE FRONT COVER. REFER TO ENGINE FRONT COVER REPLACEMENT.

O THE THREE CHAIN TENSIONERS (THE TENSIONERS MAY BE IN THEIR INSTALLED POSITIONS, BUT MUST BE FULLY RETRACTED).

O THE OIL PUMP. REFER TO OIL PUMP COVER AND GEAR SET REMOVAL.

2. THE PRIMARY AND SECONDARY CHAIN GUIDES SHOULD BE REINSTALLED IF PREVIOUSLY REMOVED.

3. ROTATE THE CRANKSHAFT UNTIL THE SPROCKET DRIVE KEY IS AT APPROXIMATELY THE 1 O'CLOCK POSITION. USE J 39946 TO ROTATE THE CRANKSHAFT.

4. INSTALL THE CRANKSHAFT AND THE INTERMEDIATE SHAFT SPROCKETS TO THE PRIMARY DRIVE CHAIN WITH THEIR TIMING MARKS ADJACENT TO EACH OTHER.

5. INSTALL THE CRANK AND INTERMEDIATE SPROCKETS OVER THEIR RESPECTIVE SHAFTS.

6. ROTATE THE CRANKSHAFT AS NECESSARY TO ENGAGE THE CRANKSHAFT KEY IN SPROCKET WITHOUT CHANGING THE RELATIONSHIP OF THE TIMING MARKS TO EACH OTHER. USE J 39946 TO ROTATE THE CRANKSHAFT.

#### NOTICE: REFER TO FASTENER NOTICE IN CAUTIONS AND NOTICES.

7. INSTALL THE INTERMEDIATE SPROCKET RETAINER BOLT.

TIGHTEN

TIGHTEN THE INTERMEDIATE SPROCKET RETAINER BOLT TO 60 N.M (44 LB FT).

8. INSTALL THE PRIMARY CHAIN TENSIONER OR RELEASE THE TENSIONER SHOE.

TIGHTEN

TIGHTEN THE TENSIONER MOUNTING BOLTS TO 25 N.M (18 LB FT).

9. INSTALL FLYWHEEL HOLDER J 39411 TO LOCK CRANKSHAFT IN THIS POSITION. IF THE ENGINE IS ON A STAND, AN ALTERNATE METHOD SHOULD BE DEVISED.

10. ROUTE THE SECONDARY DRIVE CHAIN FOR THE LH CYLINDER HEAD OVER THE INNER ROW OF INTERMEDIATE SHAFT TEETH.

#### IMPORTANT:

THE RE CAMSHAFT SPROCKET MUST CONTAIN THE CAMSHAFT POSITION SENSOR PICK-UP.

11. ROUTE THE SECONDARY DRIVE CHAIN OVER THE CHAIN GUIDE AND INSTALL THE EXHAUST CAMSHAFT SPROCKET TO THE CHAIN, SUCH THAT THE CAMSHAFT DRIVE PIN ENGAGES THE SPROCKET NOTCH MARKED LE (LEFT HEAD EXHAUST). THERE SHOULD BE NO SLACK IN THE LOWER SECTION OF THE CHAIN AND THE CAMSHAFT DRIVE PIN MUST BE PERPENDICULAR TO THE CYLINDER HEAD FACE.

12. INSTALL THE INTAKE CAMSHAFT SPROCKET INTO THE CHAIN SO THAT THE SPROCKET NOTCH MARKED LI (LEFT HEAD INTAKE) ENGAGES THE CAMSHAFT DRIVE PIN WHILE THE PIN REMAINS PERPENDICULAR TO THE CYLINDER HEAD FACE. A HEX IS CAST INTO THE CAMSHAFTS BEHIND THE LOBES FOR CYLINDER 1 (OR 2, LH) SO THAT AN OPEN END WRENCH MAY BE USED TO PROVIDE MINOR REPOSITIONING OF THE CAMSHAFTS.

13. LOOSELY INSTALL THE EXHAUST CAMSHAFT SPROCKET RETAINER BOLT.

14. LOOSELY INSTALL THE INTAKE CAMSHAFT SPROCKET RETAINER BOLT.

15. INSTALL THE CHAIN TENSIONER OR RELEASE THE TENSION ON THE SHOE.

TIGHTEN

TIGHTEN THE TENSIONER MOUNTING BOLTS TO 25 N.M (18 LB FT). TIGHTEN THE CAMSHAFT SPROCKET BOLTS TO 120 N.M (90 LB FT).

#### IMPORTANT:

THE RE CAMSHAFT SPROCKET MUST CONTAIN THE CAMSHAFT POSITION SENSOR PICK-UP.

16. ROUTE THE SECONDARY DRIVE CHAIN FOR RIGHT SIDE CYLINDER HEAD OVER OUTER ROW OF INTERMEDIATE SHAFT TEETH AND REPEAT STEPS 11 THROUGH 15 FOR RIGHT SIDE CAMSHAFTS. RIGHT SIDE CAMSHAFT SPROCKETS ARE IDENTIFIED AS RI (RIGHT INTAKE) AND RE (RIGHT EXHAUST). IN ADDITION, THE RE SPROCKET MUST CONTAIN THE CAMSHAFT POSITION SENSOR PICK-UP.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1998 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.