SMU - SECTION 8C - CUPHOLDER REPLACEMENT PROCEDURE. Cadillac Concours 1996

For 1990-2009 cars

# SMU - SECTION 8C - CUPHOLDER REPLACEMENT PROCEDURE

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 8C - CUPHOLDER REPLACEMENT PROCEDURE FOR FULL CONSOLE

#### MODELS: 1996 CADILLAC CONCOURS, DEVILLE, ELDORADO, SEVILLE

PLEASE INSERT THE FOLLOWING CUPHOLDER REPLACEMENT PROCEDURE IN SECTION 8C, PAGE 8C-17 OF THE SERVICE MANUAL.

REMOVE OR DISCONNECT:

1. OPEN CUPHOLDER.

2. RUBBER LINER FROM BOTTOM OF CUPHOLDER.

3. PHILIPS HEAD SCREWS (2) FROM BOTTOM OF CUPHOLDER.

4. CUPHOLDER FROM CONSOLE.

INSTALL OR CONNECT:

1. CUPHOLDER INTO CONSOLE.

2. PHILIPS HEAD SCREWS (2).

3. RUBBER LINER TO BOTTOM OF CUPHOLDER.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.