Oil Pump Installation. Cadillac Concours 1996

For 1990-2009 cars

#### Tools Required

J 36660-A Torque Angle Meter

1. Install the oil pump drive spacer into the oil pump so that the drive flat engages the pump rotor.
2. Position the oil pump on the crankshaft.
3. Install the retaining bolts.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Apply upward pressure on the pump while tightening the three retaining bolts. Tighten the bolts in the sequence (1, 2, 3) shown.

4.1. | First Pass

Tighten
Tighten the oil pump mounting bolts in sequence to 10 N·m (89 lb in).

4.2. | Final Pass

Tighten
Tighten the oil pump mounting bolts in sequence an additional 35 degrees using the J 36660-A .