Volt/Charge Indicator Inoperative. Cadillac Concours 1997

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---

1

1. Turn the ignition ON with the engine in RUN.
2. If the charge indicator is not on, detach the wire harness at the generator and the ground L terminal.

Does the indicator go on?

--

Go to Step 4

Go to Step 2

2

1. Check for an open in CKT 225.
2. Repair any open circuit.

Does the indicator go on?

--

Go to Starter and Charging System Check

Go to Step 3

3 | Check for a burned out indicator bulb. Replace as needed. Does the indicator go on? | -- | Go to Starter and Charging System Check | --
4 | Repair or replace the generator. Refer to Engine Electrical, Generator Replacement. Is the repair complete? | -- | Go to Starter and Charging System Check | --