Component Resistance. Cadillac Concours 1996

For 1990-2009 cars

#### 4T80-E Component Resistance Chart

Component | Pass Thru Pins | Res 20°C | Res 80°C | Res to Grd (Case)
--- | --- | --- | --- | ---
1-2 Shift Solenoid Valve | A, E | 20-30 ohms | 23-50 ohms | Greater than 250 K ohms
2-3 Shift Solenoid Valve | B, E | 20-30 ohms | 23-50 ohms | Greater than 250 K ohms
A/T Input (Shaft) Speed Sensor | S, V | 1260-1540 ohms | -- | --
TCC PWM Solenoid Valve | U, T | 10-15 ohms | 11-25 ohms | Greater than 250 K ohms
Pressure Control Solenoid | C, D | 3.5-4.6 ohms | -- | Greater than 250 K ohms
Transmission Fluid Pressure (TFP) Manual Valve Position Switch | Refer to Pressure Switch Assembly Resistance Check .
*Transmission Fluid Temperature (TFT) Sensor | M, L | 3088-3942 ohms | 159.3-198.0 ohms | Greater than 10 M ohms
Vehicle Speed Sensor | A, B VSS CONN | 1260-1540 ohms | -- | Greater than 10 M ohms
*Important: The resistance of this device is necessarily temperature dependent and will therefore vary far more than any other device. Refer to Transmission Fluid Temperature Sensor portion of Electronic Component Description .