Fastener Tightening Specifications. Cadillac Concours 1996

For 1990-2009 cars

Application | N·m | Lb Ft | Lb In
--- | --- | --- | ---
Air Conditioning Bracket to Lower Crankcase Lock Nut | 30 | 22 | --
Air Conditioning Bracket to Lower Crankcase Stud | 25 | 20 | --
Air Conditioning Compressor to Block and Bracket | 50 | 35 | --
Accessory Belt Idler Puller | 50 | 37 | --
Accessory Drive Belt Tensioner | 50 | 37 | --
Transaxle Bell Housing to Engine | 75 | 55 | --
Brace--Left Bank (Long) | 75 | 55 | --
Brace--Left Bank (Short) | 50 | 37 | --
Braces--Right Bank | 50 | 37 | --
Camshaft Bearing Cap | 12 | -- | 106
Camshaft Chain Guide Access Plug | 4.5 | -- | 39
Camshaft Cover | 10 | -- | 89
Camshaft Drive Chain Guide Bolts | 25 | 18 | --
Camshaft Drive Chain Tensioner to Block | 25 | 18 | --
Camshaft Seal Retainer to Cam Cover (Left Hand Head) | 1.1 | -- | 10
Camshaft Sprocket | 120 | 89 | --
Catalytic Converter to Exhaust Manifold Rear Pipe | 50 | 37 | --
Connecting Rod Bolt | 25 + 110 degrees | 18 + 110 degrees | --
Coolant Temp Sensor | 20 | 15 | --
Crankshaft Balancer Bolt | 50 + 120 degrees | 37 + 120 degrees | --
Crankshaft Position Sensor | 10 | -- | 89
Cruise Control Bracket to Throttle Body Bracket | 12 | -- | 106
Cylinder Head Bolt (M11)
First Pass | 40 | 30 | --
Second Pass | + 70 degrees | --
Third Pass | + 60 degrees | --
Final Pass | + 60 degrees (total 190 degrees) | --
Cylinder Head Bolt (M6) | 12 | -- | 106
Cylinder Head Plug | 80 | 59 | --
Cylinder Head Plug (Oil Gallery) | 12 | -- | 106
Cylinder Head Plug (Soc Hex) | 5.5 | -- | 49
EGR Pipe (to Water Crossover) | 28 | 21 | --
EGR Piper (Throttle Body Spacer) | 28 | 21 | --
EGR Tube to Intermediate Pipe Nut | 60 | 44 | --
EGR Valve | 25 | 18 | --
Exhaust Manifold Pipe to Cylinder Head | 25 | 18 | --
Exhaust Manifold Pipe to EGR Tube | 60 | 44 | --
Exhaust Manifold Pipe to Exhaust Manifold Rear Pipe | 30 | 22 | --
Exhaust Manifold Pipe to Lower Crankcase | 30 | 22 | --
Exhaust Manifold Rear Pipe to Right Manifold | 50 | 37 | --
Exhaust Manifold to Cylinder Head Lock Nut | 24 | 18 | --
Exhaust Manifold to Cylinder Head Bolt | 25 | 18 | --
Flywheel | 15 + 50 degrees | 11 + 50 degrees | --
Flywheel Housing Cover | 12 | -- | 106
Front Cover Bolts | 10 | -- | 89
Generator and Air Conditioning Bracket to Block | 50 | 37 | --
Generator Bracket to Block (Rear Bolt) | 47 | 35 | --
Generator Bracket to Block (Rear Nut) | 38 | 28 | --
Generator to Bracket (Front Lower Bolt) | 50 | 37 | --
Generator to Bracket (Front Upper Bolt) | 50 | 37 | --
Generator to Bracket (Rear) | 50 | 37 | --
Ignition Module (to Cam Cover) | 12 | -- | 106
Intake Manifold | 10 | -- | 89
Intermediate Sprocket Retaining Bolt | 60 | 44 | --
Intermediate Sprocket Shaft Bolts | 10 | -- | 89
Knock Sensor | 20 | 15 | --
Lift Bracket--Front | 47 | 35 | --
Lift Bracket--Right Rear | 50 | 37 | --
Lower Crankcase to Block | 30 | 22 | --
Main Bearing Bolt/Stud (In Sequence) | 20 + 65 degrees | 15 + 65 degrees | --
Mounting Bracket to Air Conditioning Compressor | 25 | 20 | --
Oil Cooler Lines to Oil Cooler | 18 | 13 | --
Oil Cooler Lines to Oil Filter Adapter | 18 | 13 | --
Oil Filter Adapter | 16 | 12 | --
Oil Filter Adapter Plug | 50 | 37 | --
Oil Level Indicator Tube | 10 | -- | 89
Oil Level Sensor | 20 | 15 | --
Oil Manifold Plate to Lower Crankcase | 10 | -- | 89
Oil Pan | 10 | -- | 89
Oil Pan Bolt

- First Pass

8

--

71

- Final Pass

12

--

106

Oil Pan Brace | 50 | 37 | --
Oil Pan Drain Plug | 20 | 15 | --
Oil Pump Suction Pipe (Lock Nut) | 25 | 18 | --
Oil Pump to Lower Crankcase | 10 + 35 degrees | -- | 89 + 35 degrees
Oxygen Sensors | 40 | 30 | --
Power Steering Pump (to Bracket) | 25 | 18 | --
Power Steering Pump Bracket (to Block) | 50 | 37 | --
Starter (to Block) | 30 | 22 | --
Starter Motor (Lock Nut) | 10 | -- | 89
Thermostat Outlet to Water Pump Cover | 10 | -- | 89
Torque Converter to Flywheel | 47 | 35 | --
Torque Strut Bracket to Cylinder Head | 50 | 37 | --
Torque Strut Bracket to Cylinder Head (Stud) | 50 | 37 | --
Torque Strut Bracket to Water Manifold | 25 | 18 | --
Water Crossover (to Block) | 25 | 18 | --
Water Crossover (to Head) | 25 | 18 | --
Water Crossover Plug | 25 | 18 | --
Water Outlet Fitting | 50 | 37 | --
Water Outlet to Head | 25 | 18 | --
Water Pump Assembly | 100 | 74 | --
Water Pump Drive Belt Tensioner to Water Crossover (Stud) | 10 | -- | 89
Water Pump Cover to Water Pump Housing | 10 | -- | 89