Neutral - Engine Running. Cadillac Concours 1996

For 1990-2009 cars

For a view of the oil flow diagram, refer to the 1996 TURM Manual.

When the gear selector lever moves to the Neutral (N) position from the Reverse (R) position, the following changes to the hydraulic and the electrical systems in the transmission occur:

### REVERSE CLUTCH RELEASES

#### Manual Valve

Mechanically controlled through the gar selector lever, the manual valve directs line pressure into the PRND43 and the PRND4 circuits. PRND4 fluid then passes around a valve land and enters the PRN fluid passage.

### Pressure Switch

Line fluid pressure, acting on the diaphragms of the PRND43 and the PRND4 pressure, closes the switches thereby completing their circuits. At the same time, reverse fluid pressure exhausts at the manual valve. This action allows the reverse pressure switch to open its circuit to the PCM. The sequence of open and closed switches at the pressure switch assembly provides the input data to the PCM, indicating the position of the manual valve.