SMU - SECTION 9J - REVISED LOCATION FOR PASSENGER. Cadillac Concours 1997

For 1990-2009 cars

# SMU - SECTION 9J - REVISED LOCATION FOR PASSENGER

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 9J - REVISED LOCATION FOR PASSENGER INFLATOR MODULE YELLOW 2-WAY CONNECTOR

#### MODELS: 1997 CADILLAC CONCOURS, DEVILLE, ELDORADO, SEVILLE

THIS BULLETIN IS BEING ISSUED TO REVISE THE LOCATION FOR THE PASSENGER INFLATOR MODULE YELLOW 2-WAY CONNECTOR REFERENCED IN THE "ENABLE THE SIR SYSTEM" AND "DISABLE THE SIR SYSTEM" PROCEDURES IN SECTION 9J OF THE SERVICE MANUAL.

THE PASSENGER INFLATOR MODULE (INFLATABLE RESTRAINT I/P MODULE) YELLOW 2-WAY CONNECTOR LOCATION CHANGED ABOUT TWO MONTHS INTO PRODUCTION. THE CHANGE WAS MADE TO MOVE THE PASSENGER INFLATOR MODULE PIGTAIL AND SIR WIRING HARNESS AWAY FROM THE HVAC AIR MIX ACTUATOR. IF YOU OPEN THE TRAP DOOR IN THE REAR OF THE I/P COMPARTMENT (GLOVE BOX) AND THE 2-WAY CONNECTOR IS NOT VISIBLE, THE I/P COMPARTMENT MUST BE REMOVED TO ACCESS THE CONNECTOR. THE CONNECTOR IS CLIPPED TO THE I/P STRUCTURE OUTBOARD OF THE I/P COMPARTMENT.

ROUTE THE PIGTAIL AND SIR WIRING HARNESS AWAY FROM THE HVAC AIR MIX ACTUATOR WHEN YOU CLIP THE 2-WAY CONNECTOR TO THE I/P STRUCTURE.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1996 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.