Fuel Pressure Regulator Replacement. Cadillac Concours 1997

For 1990-2009 cars

### Removal Procedure

Notice: Do not use compressed air to test or clean a fuel pressure regulator. Excessive air pressure can damage the fuel pressure regulator.

In order to prevent damage to the fuel pressure regulator, do not immerse the fuel pressure regulator in a cleaning solvent. Use only clean engine oil to lubricate the O-rings. In order to prevent damage to the fuel pressure regulator, DO NOT use any other type of lubricant.

1. Relieve fuel system pressure. Refer to Fuel Pressure Relief Procedure .
2. Remove the vacuum hose from the pressure regulator.
3. Clean any dirt from the fuel pressure regulator (6) retaining ring (3).
4. Remove the retaining ring (3).
5. Catch any spilled fuel using a shop towel.
6. Lift and twist the fuel pressure regulator (6) from the fuel rail socket.
7. Cover the fuel pressure regulator housing to prevent contamination from entering the fuel system.
8. Clean the fuel pressure regulator filter screen (1) with gasoline.

### Installation Procedure

Important: When servicing the fuel pressure regulator, insure that the small O-ring, large O-ring, filter screen, and O-ring backup are properly placed on the regulator.

1. Install the new O-rings on the fuel pressure regulator, if a new fuel pressure regulator is not being installed.

1.1. | Install the regulator seal O-ring (2) (small O-ring).

1.2. | Install the regulator filter (1).

1.3. | Install the regulator seal O-ring (4). (large O-ring)

1.4. | Install the O-ring back-up (5).

2. Insert the regulator into the fuel rail socket using a turning motion to properly seat the O-rings.
3. Install the retaining ring (3) on the regulator (6).
4. Install the vacuum hose to the fuel pressure regulator.
5. Turn the ignition switch ON for 2 seconds.
6. Turn the ignition switch OFF for 10 seconds.
7. Turn the ignition switch ON.
8. Check for fuel leaks.
9. Install the intake manifold top cover.

Tighten
Tighten the nuts to 2 N·m (18 lb in).

Refer to the

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

in General Information.
10. Install the negative battery cable. Refer to Battery.
11. Inspect for leaks.