No Reverse. Cadillac Concours 1996

For 1990-2009 cars

Checks | Causes
--- | ---
Case Cover | Damaged
Case Cover Gaskets | Damaged or displaced
Checkball in Piston | Missing

Driven Sprocket Support

• | Porosity or broken

• | Feed holes blocked

Driven Sprocket Support Bolts | Loose, not in grooves, mislocated
Driven Sprocket Support Seals | Leaking
Fluid Pressure | Too low
Lo/Reverse Anchor Pin | Anchor pin broken or not positioned
Reaction Carrier Shell | Missing, teeth damaged
Reverse Band | Broken, worn not anchored

Reverse Band Apply Pin

• | Too short or binding in case

• | Broken

Reverse Clutch Fiber Plates | Splines or friction material worn
Reverse Clutch Housing | Cracked
Reverse Clutch Piston | Binding in case
Reverse Clutch Piston Seals | Leaking, damaged or worn
Reverse Clutch Spring Assembly | Jammed
Reverse Clutch Steel Plates | Splines worn

Reverse Servo Piston

• | Bad seal

• | Damaged housing

Snap Ring | Out