Reverse Clutch Housing Installation. Cadillac Concours 1996

For 1990-2009 cars

#### Tools Required

J 34741-3 Input Shaft Seal Sizer

1. Remove the J 34741-3 .
2. Install the reverse clutch housing and the second sprag assembly (500-520) onto the reaction carrier assembly (604). The teeth on the reverse clutch housing must seat into the reaction sun shell. Twist the reverse housing to install and insure proper seating.
3. Install the thrust washer (436) on top of the reverse clutch housing with the tabs pointing down.