Brake Transmission Shift Interlock Solenoid Replacement. Cadillac Concours 1997

For 1990-2009 cars

### Removal Procedure

1. Remove the transmission range control knob and the console trim plate.
2. Remove the electrical connector.
3. Remove the BTSI solenoid at the range control lever assembly.

### Installation Procedure

1. Install the BTSI solenoid at the range control lever assembly.
2. Install the electrical connector.
3. Install the console trim plate and the transmission range control knob.