HEADLINER FALLING DOWN IN REAR AREA AROUND FIBER OPTIC LAMP. Cadillac Concours 1994

For 1990-2009 cars

# HEADLINER FALLING DOWN IN REAR AREA AROUND FIBER OPTIC LAMP

#### SUBJECT: HEADLINER FALLING DOWN IN REAR AREA AROUND FIBER OPTIC LAMP MONITOR (REPLACE LAMP MONITOR HOUSING)

#### MODELS: 1994 CADILLAC CONCOURS AND DEVILLE

#### CONDITION:

SOME OWNERS MAY COMMENT ON THE HEADLINER FALLING DOWN IN THE REAR AREA AROUND THE FIBER OPTIC LAMP MONITOR.

#### CORRECTION:

REPLACE THE FIBER OPTIC LAMP MONITOR HOUSING WITH P/N 3548507.

PROCEDURE -

1. LOOSEN UPPER REAR SAIL PANEL ON BOTH SIDES, 3 PUSH PINS EACH.

2. REMOVE ASSIST STRAPS ON BOTH SIDES, 2 TORX SCREWS EACH.

3. REMOVE FIBER OPTIC LAMP MONITOR INTERIOR TRIM.

4. LOWER REAR OF HEADLINER AS NEEDED FOR REMOVAL OF HOUSING.

5. REMOVE FIBER OPTIC CABLES.

6. REMOVE REAR LAMP MONITOR ASSEMBLY, 1 CLIP.

7. REVERSE STEPS FOR INSTALLATION.

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: R3573 USE PUBLISHED LABOR OPERATION TIME.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.