Vehicle Speed Sensor and Transmission Fluid Cooler Pipe Fitting Installation. Cadillac Concours 1996

For 1990-2009 cars

1. Inspect the output speed sensor (130) for damage or a cut seal (4).
2. Inspect the cooler connector (3) for damaged threads, clogging, or a cut seal (4).
3. Install the output speed sensor (130) and the seal (4) into the case extension.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the output speed sensor bolt (131).

Tighten
Tighten the bolt to 8-14 N·m (6-10 lb ft).

5. Install the cooler fitting (3) and the new seal (4) into the case.

Tighten
Tighten the cooler fitting to 25-29 N·m (19-21 lb ft).