Info - Recommended Wheel Nut/Bolt Torque Specifications. Cadillac Evoq 2003

For 1990-2009 cars

# Info - Recommended Wheel Nut/Bolt Torque Specifications

Subject: | Recommended Wheel Nut/Bolt Torque Specifications

Models: | 2003 Passenger Cars and Light Duty Trucks

| 2003 HUMMER H1, H2

This bulletin is being issued to list the recommended wheel nut/bolt torque specifications for passenger cars and light duty trucks for the 2003 model year.

#### 2003 Passenger Cars

Vehicle | Fasteners | Bolt Circle Diameter (mm) | Lugwrench Hex Size | Service Torque
--- | --- | --- | --- | ---
| Number | Size |  |  | N·m | lb ft
J | 5 | M12 x 1.5 | 100 | 19 mm | 140 | 100
B, C, D, G, H, K, N, U Van, W | 5 | M12 x 1.5 | 115 | 19 mm | 140 | 100
Corvette | 5 | M12 x 1.5 | 120.65 | 19 mm | 140 | 100
Pontiac Vibe | 5 | M12 x 1.5 | 100 | 21 mm | 103 | 76

#### 2003 Light Duty Trucks

Vehicle and Application | Fasteners | Bolt Circle Diameter (mm) | Lugwrench Hex Size | Service Torque
--- | --- | --- | --- | ---
| Number | Size |  |  | N·m | lb ft
S/T (All) | 5 | M12 x 1.5 | 120.65 | 19 mm | 140 | 100
GMT360/370 (All) | 6 | M12 x 1.5 | 127 | 19 mm | 140 | 100
M/L (All) | 6 | M14 x 1.5 | 139.7 | 22 mm | 190 | 140
G/H10 (All) | 6 | M14 x 1.5 | 139.7 | 22 mm | 190 | 140
G20, 30 (All) | 8 | M14 x 1.5 | 165.1 | 22 mm | 190 | 140
C/K 15 (All Except 1500HD) | 6 | M14 x 1.5 | 139.7 | 22 mm | 190 | 140
C/K 1500HD, 25, 35 & 36 (Including Dual Wheels) | 8 | M14 x 1.5 | 165.1 | 22 mm | 190 | 140
HUMMER H1 | 8 | 9/16-18 | 165.1 | 7/8 in | 190 | 140
HUMMER H2 | 8 | M14 x 1.5 | 165.1 | 22 mm | 190 | 140
Tracker (All) | 5 | M12 x 1.25 | 139.7 | 19 mm | 95 | 69
* -- Dual wheel trucks - torque specifications apply to front and rear wheels.