For 1990-2009 cars

# COLD ENGINE KNOCK-PISTON SLAP NEW PISTON/LINER ASSY. AVAIL.

#### SUBJECT: COLD ENGINE KNOCK - PISTON SLAP (NEW PISTON/LINER ASSEMBLY)

#### VEHICLES AFFECTED: 1990-91 C,E,K WITH 4.5L - VIN 8

Some 1990-1991 DeVilles, Fleetwoods, Eldorados, and Sevilles with 4.5L and 4.9L V8 engines may exhibit a light engine knocking sound when first started during cold weather. As the engine warms to operating temperature, the noise becomes quieter and may eventually disappear.

To repair this condition install a new piston/liner assembly, P/N 3534204. This kit has a revised piston skirt contour and a thicker wall cylinder liner. The revised part number should be used to replace only those assemblies exhibiting the noise condition.

For vehicles repaired under warranty use Labour Operations J1300, J1301, or J1307 as required.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.