For 1990-2009 cars

# SMU - SECTION 7 - LOAND REVERSE CLUTCH SPACER

REVISION: 09/06/95

THIS BULLETIN IS BEING REVISED TO INCLUDE THE 4L60 TRANSMISSION. PLEASE DISCARD BULLETIN 57-71-12 (SECTION 7 - TRANSMISSION). ----------------------------------------------------------------------

#### SUBJECT: SERVICE MANUAL UPDATE-SECTION 7-LO AND REVERSE CLUTCH SPACER PLATE SELECTION

#### MODELS: 1993-95 BUICK ROADMASTER 1993-95 CADILLAC FLEETWOOD 1993-95 CHEVROLET CAMARO, CAPRICE, CORVETTE 1993-95 PONTIAC FIREBIRD

1993-95 CHEVROLET AND GMC TRUCK C/K, S/T, M/L, G MODELS 1993-94 OLDSMOBILE BRAVADA WITH 4L60/4L60-E TRANSMISSION (RPOS M30, MD8)

THE DIMENSION 'D' FOR THE OVERALL HEIGHT FOR THE LO REVERSE CLUTCH PLATES IS IN ERROR. THE CORRECT MEASUREMENT SHOULD BE 29.22 TO 29.90 MM (1.15 TO 1.18 INCHES).

ATTACHED ARE THE UPDATED PAGES FOR YOUR SERVICE MANUAL.

FIGURES: 0 ATTACHMENTS: 2

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.