For 1990-2009 cars

# INFO ON WHEEL ALIGNMENT SPECS. (REVISED SPECIFICATIONS)

#### SUBJECT: INFORMATION ON WHEEL ALIGNMENT SPECIFICATIONS

VEHICLES AFFECTED: 1992 C,E,K AND V MODELS ------------------

Wheel alignment specifications were changed at the start of production. The following chart is to revise wheel alignment specifications that were published in the 1992 Service Information Manual (Section 3A).

#### WHEEL ALIGNMENT SPECIFICATIONS

FRONT CASTER 2.3 DEG. +/- 1.0 DEG. CROSS CASTER (L - R) 0.0 DEG. +/- 1.0 DEG. CAMBER - LEFT -0.5 DEG. +/- 0.5 DEG. CAMBER - RIGHT +0.5 DEG. +/- 0.5 DEG. CROSS CAMBER (L - R) -1.0 DEG. +/- 0.6 DEG. TOE PER WHEEL 0.1 DEG. +/- 0.1 DEG. SUM TOE (L + R) 0.2 DEG. +/- 0.2 DEG. STEERING WHEEL ANGLE 0.0 DEG. +/- 2.5 DEG.

REAR TOE PER WHEEL 0.1 DEG. +/- 0.1 DEG. SUM TOE (L + R) 0.2 DEG. +/- 0.2 DEG. THRUST ANGLE 0.0 DEG. +/- 0.1 DEG.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.