For 1990-2009 cars

# FRONT SEAT BACK CUSHION TILTED OUTBOARD

FRONT SEAT BACK CUSHION TILTED OUTBOARD

#### VEHICLES AFFECTED: 1985-1988 DEVILLES AND FLEETWOODS -----------------

Some 1985-1988 DeVilles and Fleetwoods may experience a condition of front seats leaning outboard. To repair this condition, use the following procedure:

1. Raise seat to full up position.

2. Disconnect drive cable from rear vertical gear nut on inboard side, refer to Figures 1 and 2.

3. Move rear tilt down, using the door-mounted control switch, until seat is no longer leaning.

4. Reconnect drive cable.

Use the most applicable labour operation from the Canadian Labour Time Guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.