For 1990-2009 cars

# WARPED FRT. OR REAR DOOR PULL HANDLE TRIM PANEL INSERT

#### VEHICLES AFFECTED: 1986-87 CADILLAC BROUGHAMS (D)

A BUCKLED OR WARPED FRONT OR REAR DOOR PULL HANDLE TRIM PANEL INSERT (FIGURE 1) MAY BE ENCOUNTERED ON SOME 1986 AND 1987 BROUGHAMS. THIS CONDITION CAN BE REPAIRED BY USING THE FOLLOWING PROCEDURE.

1. REMOVE DOOR TRIM PANEL AS SPECIFIED IN THE 1986 BODY SERVICE MANUAL, PAGE 5B-3.

2. REMOVE PULL HANDLE ASSEMBLY.

3. FABRICATE A METAL BRACKET (33mm X 20MM X IMM) AS SHOWN IN FIGURE 2.

4. POSITION NEW BRACKET OVER STUDS THAT ATTACH THE "CREST" TO THE TRIM PANEL INSERT (FIGURE 3).

5. INSTALL TWO SMALL SPRING STEEL CL,IPS (P/N 9428633) OVER "CREST" STUDS.

6. REINSTALL TRIM.

Use the most applicable labour operation from the Canadian Labour Time Guide and claim 0.5 hours.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.