For 1990-2009 cars

# ABS SYSTEM USAGE REFERENCE FOR ALL CADILLAC MODELS

#### SUBJECT: ABS SYSTEM USAGE REFERENCE FOR ALL CADILLAC MODELS

#### VEHICLES AFFECTED: 1986-91 C,D,E,K,V

Cadillac has used several different ABS systems since 1986. The attached reference card includes for each vehicle the system used, the type of diagnostics available, and the special tools required.

This card is intended for ready reference only and in no way replaces the service and diagnostic information published in Section 5 of the applicable Service Information Manual.

#### ABS SYSTEM USAGE FOR ALL CADILLAC MODELS

DIAGNOSIS SPECIAL TOOLS REQUIRED --------- ---------------------- ELDORADO/ SEVILLE --------- 1988 IGN OFF, GROUND PIN "G" OF J-35592 PINOUT BOX TEVES MARK II THE ALDL, TURN IGN ON TO J-35604 PRESSURE GAGE FLASH THE ABS CODES. DRIVE J-35804 PRESSURE SWITCH SOCKET VEHICLE OVER 18 MPH TO CLEAR J-35798 BLEEDER ADAPTER CODES

1989- IGN OFF, GROUND PIN "H" OF J-35592 PINOUT BOX 1990 THE ALDL, TURN IGN ON TO J-35604-88 PRESSURE GAGE ADAPTER TEVES MARK II FLASH THE ABS CODES. DRIVE J-35604 PRESSURE GAGE VEHICLE OVER 18 MPH TO CLEAR J-35804 PRESSURE SWITCH SOCKET CODES J-35798 BLEEDER ADAPTER

1991 IGN OFF, GROUND PIN "H" OF J-35592 PINOUT BOX BOSCH 2U THE ALDL, TURN IGN ON TO TECH1 FLASH THE ABS CODES. USE THE TA00022 BOSCH ABS ADAPTER TECH1 TO MONITOR ABS DATA. TKO3030A 1988-91 BRAKE CARTRIDGE A-H JUMPER

#### BROUGHAM

1990- IGN OFF, GROUND PIN "H" OF J-35592 PINOUT BOX 1991 THE ALDL, TURN IGN ON TO TECH1 BOSCH 2U FLASH THE ABS CODES. USE THE TA00022 BOSCH ABS ADAPTER TECH1 TO DISPLAY CODES AND TKO3030A 1988-91 BRAKE CARTRIDGE ABS DATA. A-H JUMPER

#### ALLANTE

1987- FLASH ABS CODES BY J-35592 PINOUT BOX 1989 DEPRESSING BRAKE PEDAL J-35592-OLY (OVERLAY) BOSCH ABS III WHILE IN DIAGNOSTICS J-35210-90 HARNESS ADAPTER (SERVICE MODE)

1990- BCM CODES B480 AND B483. IGN J-36210 ABS TESTER 1991 OFF, GROUND PIN "H" OF THE J-35604 PRESSURE GAGE BOSCH ABS III ALDL, TURN IGN ON TO FLASH J-35798 BLEEDER ADAPTER WITH TRACTION THE ABS CODES. J-35604-25 ADAPTER CONTROL (TCS) A-H JUMPER

DE VILLE/ FLEETWOOD --------- 1986 LIGHT SEQUENCE J-35592 PINOUT BOX TEVES MARK II DETERMINATION J-35604 PRESSURE GAGE (SPEED RING REFER TO SERVICE MANUAL J-35804 PRESSURE SWITCH SOCKET HAS 96 TEETH) PAGE 5El-4

1987- LIGHT SEQUENCE J-35592 PINOUT BOX 1988 DETERMINATION J-35604 PRESSURE GAGE TEVES MARK II REFER TO SERVICE MANUAL J-35804 PRESSURE SWITCH SOCKET (SPEED RING PAGE 5El-4(1987) J-35798 BLEEDER ADAPTER HAS 47 TEETH) REFER TO SERVICE MANUAL PAGE 5E-13(1988)

1989- IGN OFF, GROUND PIN "H" OF J-35592 PINOUT BOX 1990 THE ALDL TURN IGN ON TO J-35604-88 PRESSURE GAGE ADAPTER TEVES MARK II FLASH THE ABS CODES. DRIVE J-35604 PRESSURE GAGE VEHICLE OVER 18 MPH TO CLEAR J-35804 PRESSURE SWITCH SOCKET CODES J-35798 BLEEDER ADAPTER

1991 NO FLASH CODES. TECH1 FOR J-38716 PINOUT BOX TEVES MARK IV CODE DISPLAY AND TO TECH1 MONITOR ABS DATA TKO3030A 1988-91 BRAKE CARTRIDGE

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.