For 1990-2009 cars

# CLUSTER DISASSEMBLY SERVICE MANUAL ADDITION

#### VEHICLES AFFECTED: 1985 Oldsmobile Ninety-Eight

Whenever it becomes necessary to disassemble the cluster in a 1985 Ninety-Eight for repairs, the following procedures and Fig. -- should be added to the cluster removal procedures on Page 8C4-8 of the 1985 Firenza, Calais, Cutlass Ciera and Ninety-Eight Chassis Service Manual, Volume II.

1. Remove cluster lens and retainer.

2. Remove speedometer attaching screws.

3. Carefully lift speedometer and disconnect odometer connectors.

The speedometer head and circuit board can now be sent to the speedometer repair centre, if required.

4. Remove gauges attaching screws.

5. Lift gauges out.

6. Remove trip odometer attaching screws.

7. Remove stepper motor from odometer assembly.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.