For 1990-2009 cars

# DOOR INTERIOR PULL HANDLE DISENGAGEMENT

#### VEHICLES AFFECTED: 1985 Cadillac FWD Devilles and Fleetwoods -----------------------------------------

The front and/or rear door interior pull handles could disconnect from the trim plate (refer to Figure 1) nn some 1985 front-wheel-drive Devilles and Fleetwoods. A revised roll pin (P/N 11508684) has been released for production and is currently available through the Parts Department to service vehicles experiencing this condition.

To install the now 12.7mm (1/2 in.) pin, follow the listed service procedure:

1. Remove pull handle assembly from door an dencribed in Section 5 of the Body Service Manual, (Door Trim Panel and Applique Removal).

2. Remove spring (1) from the back of door handle assembly.

3. Remove 9.5mm (3/8 in.) roll pins (2),

4. Insert 12.7mm (1/2 in.) replacement roll pins (P/N 11508684).

5. Reinstall spring.

6. Reinstall pull handle assembly onto the door.

Use the most applicable labour operation from the Canadian Labour Time Guide and claim 0.7 hours.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.