For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle.
2. Remove the access panel.
3. Disconnect the hoses from the canister.
4. Remove the canister (2) from the canister bracket.
5. Remove the canister (2) from the vehicle.

### Installation Procedure

1. Install the canister (2) to the bracket .
2. Connect the hoses to the canister (2).
3. Install the access panel.
4. Lower the vehicle.