For 1990-2009 cars

# A/C R-12 SERVICE PROCEDURES CHARGING CAPACITY CHART

To assist in assuring proper charge during service procedures, the following chart has been printed and laminated for easy reference. Two charts are included for attachment to your charging station. Limited supplies will be available through your zone offices if additional copies are needed.

#### NOTE: These capacities may not be applicable for limousines or custom coaches with rear A/C.

#### MODEL DE VILLE BROUGHAM CIMARRON ALLANTE ELDORADO YEAR FLEETWOOD -------- -------- ------- SEVILLE ---- --------- ------- 1985 2 7/8 LBS. 3 1/2 LBS. 2 1/4 LBS. 3 1/2 LBS.

1986 2 1/2 LBS. 3 1/2 LBS. 2 1/4 LBS. 2 3/4 LBS.

1987 2 3/8 LBS. 3 1/2 LBS. 2 1/4 LBS. 2 1/4 LBS. 2 3/4 LBS.

1988 2 3/8 LBS. 3 1/2 LBS. 2 1/4 LBS. 2 1/4 LBS. 2 3/8 LBS.

1989 2 7/8 LBS. 3 1/3 LBS. 2 1/4 LBS. 2 3/8 LBS.

1990 2 7/8 LBS. 3 1/3 LBS. 2 1/4 LBS. 2 3/8 LBS.

Figure 1 Cadillac R-12 Charging Capacity Table

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.