For 1990-2009 cars

# 1-2 SHIFT SHUDDER-THM 440-T4 REPAIR PROCEDURE

#### MODELS AFFECTED: 1985-1987 DE VILLE, AND 1986-1987 ELDORADO AND SEVILLE

Some production and SRTA THM440-T4 transaxles built prior to April 15, 1987 (Julian Date 105), may exhibit a 1-2 upshift shudder during li t to moderate acceleration. This condition may be caused by out of flat (thickness variation clutch plates. To repair this condition, replace the 2nd clutch plates with the service package described below. When servicing a transaxle for 1-2 shift shudder or performing any operation for which an overhaul package is used, discard the fiber plates from the package and the original steel and fiber plates from the 2nd clutch assembly. Use the appropriate service package listed below.

Part Number Application ----------- ----------- 8662914 Six fiber and six steel plates for 1987 transales

8662913 Five fiber and five steel plates for 1985-1986 transaxles

#### NOTICE: 1987 steel plates are .075" thick. 1985 & 1986 steel plates are .088" thick. Do NOT interchange these plates.

Refer to the Service Information Manual Unit Repair section for Second Clutch Service Information and Procedure.

For warranty purposes, use Labor Operation K7535 at 6.0 hours for DeVille/Fleetwood and 6.6 hours for Eldorado and Seville.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.