For 1990-2009 cars

# SMU - SECTION 6A - ENGINE MECHANICAL

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 6A - ENGINE MECHANICAL - NEW J TOOL APPLICATION

#### MODELS: 1994-96 BUICK ROADMASTER 1994-96 CADILLAC FLEETWOOD 1992-96 CHEVROLET CORVETTE 1993-96 CHEVROLET CAMARO 1994-96 CHEVROLET CAPRICE, IMPALA SS 1993-96 PONTIAC FIREBIRD WITH 4.3L AND 5.7L ENGINES (VINS W, P - RPOS L99, LT1)

THIS BULLETIN PROVIDES UPDATED INFORMATION REGARDING SPECIAL TOOLS.

NEW J TOOL 41546 CAN BE USED TO SERVICE ALL WATER PUMP DRIVESHAFT ASSEMBLIES. J TOOL 39092 CAN ONLY BE USED TO SERVICE 1992 AND 1993 V8 LT1 APPLICATIONS.

FIGURES: 0 ATTACHMENTS: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.