For 1990-2009 cars

# FRONT SEAT CENTER ARMREST DOOR FALLS OPEN

#### SUBJECT: FRONT SEAT CENTER ARMREST DOOR FALLS OPEN (INSTALL HOOK AND LOOP MATERIAL)

#### MODELS: 1993-94 BUICK ROADMASTER 1993-94 CADILLAC FLEETWOOD

#### CONDITION:

SOME OWNERS MAY COMMENT THAT THE CENTER ARMREST LID COMES OPEN WHEN STORED IN THE VERTICAL POSITION.

#### CORRECTION:

INSTALL A LENGTH OF 3M HOOK AND LOOP P/N 06480 OR EQUIVALENT USING THE FOLLOWING PROCEDURE.

1. FOLD CENTER ARMREST/STORAGE BOX DOWN AND OPEN COMPARTMENT LID AS ILLUSTRATED IN FIGURE 1.

2. CUT A 3-1/2 INCH PIECE OF 3M HOOK AND LOOP MATERIAL AND APPLY IT TO THE REAR EDGE OF THE STORAGE BOX AND LID AS INDICATED IN FIGURE 1, ITEM 1.

#### NOTE: OWNERS SHOULD BE CAUTIONED NOT TO OVER FILL THE STORAGE BOX.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE: LABOR OPERATION: T3412 LABOR TIME: 0.2 HR.

FIGURES: 1

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1993 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.