For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle.
2. Disconnect the Crankshaft Position (CKP) sensor electrical connector.
3. Remove the CKP sensor retaining screw.
4. Remove the CKP sensor.

### Installation Procedure

1. Install the crankshaft position sensor.
2. Install the crankshaft position sensor retaining screw.

Tighten
Tighten the CKP sensor to 4-6 N·m (35-53 lb in).

3. Connect the electrical connector.