For 1990-2009 cars

# DISPLAYS BLANK INTERMITTENLY ON COLD START UPS

#### MODELS AFFECTED: 1988 DE VILLES AND FLEETWOODS

Some 1988 DeVilles and Fleetwoods may experience a condition of all displays blanking during cold ambient temperatures for only a few minutes after start up. This condition may be caused by an intermittent open in the Retained Accessory Power (RAP) relay #2. To repair this condition replace the relay.

For warranty purposes use Labor Operation N2895 at .2 hour.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.