For 1990-2009 cars

# A/C R-12 SERVICE PROCEDURES CHARGING CAPACITY CHART

#### VEHICLES AFFECTED: 1985-90 CADILLAC, C,E,K,J,V AND D

To assist in assuring proper charge during service procedures the following chart has been printed for easy reference. Please attach to your charging station.

#### MODEL DEVILLE BROUGHAM CIMARRON ALLANTE ELDORADO YEAR FLEETWOOD SEVILLE ---- ---------- --------- --------- ------- ------- 1985 2 7/8 LBS. 3 1/2 LBS. 2 1/4 LBS. 3 1/2 LBS.

1986 2 1/2 LBS. 3 1/2 LBS. 2 1/4 LBS. 2 3/4 LBS.

1987 2 3/8 LBS. 3 1/2 LBS. 2 1/4 LBS. 2 1/4 LBS. 2 3/4 LBS.

1988 2 3/8 LBS. 3 1/2 LBS. 2 1/4 LBS. 2 1/4 LBS. 2 3/8 LBS.

1989 2 7/8 LBS. 3 1/3 LBS. 2 1/4 LBS. 2 3/8 LBS.

1990 2 7/8 LBS. 3 1/3 LBS. 2 1/4 LBS. 2 3/8 LBS.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.