For 1990-2009 cars

# GAP BETWEEN INSTR. PANEL UPPER TRIM PAD & INSTR. PANEL ASSEM.

#### MODELS AFFECTED: 1989 DE VILLES AND FLEETWOODS EQUIPPED WITH SUPPLEMENTAL INFLATABLE RESTRAINT (OOPTION AJ3)

Some 1989 DeVilles and Fleetwoods equipped with Supplemental Inflatable Restraint (SIR) may experience a condition of excessive gap below the left hand A/C outlet between the instrument panel upper trim pad and instrument panel assembly.

To repair the gap between the left side upper trim panel and instrument panel assembly use the following procedure:

1. Remove upper trim pad. Refer to appropriate Service Information Manual.

2. Install push-in nut, P/N 1355003, to instrument panel assembly at side attachment point. Refer to Figure 1.

3. Reinstall upper trim pad per service procedure EXCEPT use bolt/screw P/N 20365259 in place of 11500677 at left attachment location only. Refer to Figure 1.

Parts are currently available from GMSPO.

WARRANTY INFORMATION VEHICLE SERIES -------------------- Operation Operation Description Number C D E J K V ---------------------- ------ - - - - - - Cover, Instrument Panel Upper - R&R or Replace Upper C2362 .3

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.