For 1990-2009 cars

# CRANKING MOTORS - SERVICING TORQUE SPECIFICATIONS

SCREW AND BOLT TORQUE SPECIFICATIONS FOR 5MT, 10MT, 15MT/GR, 20MT, 22MT, 25MT AND 27 MT CRANKING MOTORS: TO OBTAIN OPTIMUM PERFORMANCE AND MAXIMUM SERVICE LIFE AFTER MOTOR REPAIR OR OVERHAUL, TIGHTEN FASTENERS DURING ASSEMBLY TO THE TORQUE VALUES LISTED BELOW. TORQUE FASTENER DESCRIPTION SIZE (POUND-INCHES) BRUSH SCREWS, GUIDE (5MT) 3.5 X 1.15 9 SWIVEL HOLDER 8 X 18 14 STEEL SWIVEL HOLDER 8 X 32 11 POLE SHOE SCREWS 3/8 X 24 400 SOLENOID MOUNTING SCREWS 1/4 X 20 68 THRU BOLTS, (5MT) 10 X 24 40 (5MT)AFTER DATE CODE 9013 1/4 X 20 75 (OTHER) 1/4 X 20 75 MOTOR TERMINAL SCREW 10 X 32 40 SHIFT LEVER BOLT 5/16 X 18 75 MIDDLE BEARING SCREWS 10 X 32 40 INTERNAL CONNECTOR SCREW 10 X 32 15 GEAR HOUSING MOUNTING SCREWS 1/4 X 20 85

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.