EXHAUST BOOM (NOISE) NEW HANGER BRACKET KIT. Cadillac Limousine 1986

For 1990-2009 cars

# EXHAUST BOOM (NOISE) NEW HANGER BRACKET KIT

#### VEHICLES AFFECTED: 1985-1986 Devilles and Fleetwoods

Some Devilles and Fleetwoods equipped with an HT4100 engine may experience an exhaust boom (noise) between 1830 - 1890 RPM.

To repair this condition, a new exhaust hanger bracket kit (P/N 25527855) has been developed. Vehicles which experience this condition should be serviced using the following procedure:

1. Verify the exhaust boom is present with A/C off.

2. If boom is not present with A/C off, see Product Service Bulletins 85-1-101 and 85-1-104 for A/C system diagnosis.

3. Clamp the new hanger to the tailpipe as shown in Figure 1. The weld-nut on the hanger assembly should line up with the centerline of the muffler.

4. Position the leading edge of the new body mounted exhaust hanger bracket against the old exhaust hanger bracket keeping the bottom edge flush with the bottom of the frame rail. Drill three 8mm (5/16 in.) diameter holes in frame using bracket as a guide and secure with the three self-tapping screws included in the kit.

5. Support the exhaust system and remove the original insulator and attaching bolts. Cut the point from the top bolt to shorten it to 10mm (13/32 in.) of thread length.

6. Reinstall the insulator at the new location.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.