MOTOR VEHICLE REGISTRATION DATA FOR 1985 VEHICLES. Cadillac Limousine 1985

For 1990-2009 cars

# MOTOR VEHICLE REGISTRATION DATA FOR 1985 VEHICLES

1985 Cadillac Motor Vehicle Registration Data: Devilles, Fleetwoods, Limo & Comm. Body/Chassis

Cadillac Vehicle Description - Weights - Wheelbase - Engine Data

Series Name V.I.N. Body Body No. Engine Shiping Weight ----------- Designtor Type Pass Code Killograms Pounds --------- ---- ---- ---- ---------- ------

Fleetwood B-47 2 Door S 1482.2 3268 Coupe (FWD) Coupe T 1504.0 3316

Fleetwood B-69 2 Door S 1516.5 3343 Sedan (FWD) Sedan T 1531.7 3377

Deville D-47 2 Door S 1472.2 3246 Coupe (FWD) Coupe 6 T 1492.7 3291

Deville D-49 4 Door S 1504.8 3318 Sedan (FWD) Sedan T 1514.9 3340

Fleetwood H-23 4 Door 8 S 1589.7 3505 Limousine (FWD) Limousine

Commercial A-90 - - S - - Body/Chassis (FWD)

Series Name V.I.N. Body Wheelbase Engine CU. In. ----------- Designtor Millmeters Inches Displacement --------- ---------- ------ ------------

Fleetwood B-47 Coupe (FWD)

Fleetwood B-69 Engine Code 8 - Sedan (FWD) V8-249 Cl.In. Digital 2815 110.8 Fuel Injection (DFI) Deville D-47 Coupe (FWD) Engine Cote T- Deville D-49 V6-262 Cu.In. Diesel Sedan (FWD)

Fleetwood H-23 3415 134.4 Limousine (FWD)

Commercial A-90 3715 146.3 Body/Chassis (FWD)

All weights include automatic transaxle, power steering, power brakes, and air conditioning which are standard on all vehicles. Production weights may vary slightly. Please note taxable horsepower is 39.5 for the 262 cu.in. engine, and 38.4 for the 250 cu.in engine. See engine codes below.

Engine Specifications

Displacement Cylinder Net Horsepower Fuel Cu.In. Liters Arrangement (SAE J-245) System ------- ------ ----------- ----------- ------

249 4.1 V-6 Digital Fuel Digital Injection 93(LW) 125 HP Fuel Injection

262 4.3 V-6 Diesel 63(KW) 85 HP Diesel

Displacement Engine Bore and Stroke Cu.In. Liters Code Millimeters Inches ------- ------ ---- ------------ ------

249 4.1 8 88.0 X 84.0 3.46 X 3.31

262 4.3 T 103.x 86.0 4.057 x 3.385

Cadillac Vehicle Identification Number Information

Each 1985 Cadillac carries a 17 digit Vehicle Identification number used for license and insurance identification and in general reference to the automobile. The number is located on a plate riveted to the windshield lower frame at the driver's side of the car where it is visible through the windshield. The 1985 Cadillac Vehicle Identification is decoded as follows:

1 - Nation of origin - 1 denotes USA G - manufacturer - G denotes General Motors 6 - Make "6" Denotes Cadillac C - Carline D - Series D-Deville (FWD) G-Fleetwood (FWD) H-Limousine (FWD) Z-Commercial Chassis (FWD) 00-Body type restraint system (active) 8 - Engine Code "8" denotes 249 Cu In with digital fuel injection 4.1 liters "t" denotes 262 Cu In Diesel - 4.3 Liters X - Check digit F - Model Year (F = 1985) 4 = Assemlby Plant (4 - Orion, Michigan) 200001 - Production sequence number 200001 FWD C-Orion

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.