FRONT DOOR WINDOW WILL NOT RAISE TO UP POSITION. Cadillac Limousine 1985

For 1990-2009 cars

# FRONT DOOR WINDOW WILL NOT RAISE TO UP POSITION

#### MODELS AFFECTED: 1985 DE VILLE AND FLEETWOODS

The front door windows may not raise to the full up position on some 1985 De Villes and Fleetwoods. This condition may be caused by the glass guide to regulator breaking or running out of the lower sash channel. To repair this condition relocate the rear section of the window regulator guide using the following procedure:

1. Remove door trim panel and water deflector as described in Section 5 of the 1985 FWD "C" Body Service Manual.

2. Using a 1 /4" drill bit, drill out rivets from upper and lower guide mounts of regulator guide, see Figure 1.

3. Locate and drill new regulator guide mount holes as shown in Figure 1.

4. Install guide into lower sash channel, as described in Section 5 of the 1985 FWD "C" Body Service Manual, if broken or disengaged from lower sash channel.

5. Reposition regulator guide over new guide mounting holes and attach to door inner panel with 1 /4" peel type rivets.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.