LOOSE DOOR WINDOW SWITCH PLATE REPAIR PROCEDURE. Cadillac Limousine 1985

For 1990-2009 cars

# LOOSE DOOR WINDOW SWITCH PLATE REPAIR PROCEDURE

#### MODELS AFFECTED: 1995 DE VILLES AND FLEETWOODS

This bulletin supersedes Serviceman Bulletin 85-57, Group 10, which should be destroyed.

Door window switch plate escutcheons (wood grain appliques) which may become toose from the switch plate base may be repaired as follows:

1. Thoroughly clean the cementing surfaces using 3M-8984 or equivalent solvent.

2. Recement switch plate escutcheon to switch plate base using 3M-8101 structural adhesive, Loctite Quick Jel (SGGA) or equivalent, recement escutcheon to switch plate base. Follow adhesive manufacturer's label directions for bonding.

For warranty purposes, use Labor Operation No. T0131 at .3 hour per door.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.