DTC P0719 Brake Switch Circuit Low Input. Chevrolet Brazil Blazer 1997

For 1990-2009 cars
Automatic Transmission Components 4.3L
Automatic Transmission Controls Schematics 4.3L
OBD II Symbol Description Notice
Handling ESD Sensitive Parts Notice

### Circuit Description

The brake switch indicates the brake pedal status. The brake switch is normally-closed. The brake switch supplies a B+ signal on circuit 420 to the VCM. The signal voltage circuit is opened when you apply the brakes. The VCM uses this signal in order to de-energize the TCC Sol. Valve when you apply the brakes.

When the VCM detects an open brake switch circuit during accelerations, then DTC P0719 sets. DTC P0719 is a type A DTC.

### Conditions for Setting the DTC

• | No VSS Assy. DTC P0502.

• | The VCM detects an open brake switch or circuit (0 volts) for 15 minutes without changing for 2 seconds, and the following events occur seven consecutive times:

- | The vehicle speed is less than 8 km/h (5 mph);

- | then the vehicle speed is 8-32 km/h (5-20 mph) for 4 seconds;

- | then the vehicle speed is greater than 32 km/h (20 mph) for 6 seconds.

### Action Taken When the DTC Sets

• | The VCM inhibits 4th gear if the transmission is in hot mode.

• | The VCM freezes shift adapts from being updated.

• | The VCM illuminates the Malfunction Indicator Lamp (MIL).

### Conditions for Clearing the MIL/DTC

• | The VCM turns OFF the MIL after three consecutive ignition cycles without a failure reported.

• | A scan tool can clear the DTC from the VCM history. The VCM clears the DTC from the VCM history if the vehicle completes 40 warm-up cycles without a failure reported.

• | The VCM cancels the DTC default actions when the fault no longer exists and the ignition is OFF long enough in order to power down the VCM.

### Diagnostic Aids

• | Inspect the wiring for poor electrical connections at the VCM. Inspect the wiring for poor electrical connections at the brake switch. Look for the following conditions:

• | A bent terminal

• | A backed out terminal

• | A damaged terminal

• | Poor terminal tension

• | A chafed wire

• | A broken wire inside the insulation

• | When diagnosing for an intermittent short or open condition, massage the wiring harness while watching the test equipment for a change.

• | Ask about the customer's driving habits. Ask about unusual driving conditions (e.g. stop and go, expressway, etc.).

• | Inspect the brake switch for proper mounting and adjustment.

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. This step isolates the brake switch as a source for setting the DTC.

#### DTC P0719 Brake Switch Circuit -- Low Input

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Powertrain On-Board Diagnostic (OBD) System Check performed? | -- | Go to Step 2 | Go to A Powertrain On Board Diagnostic (OBD) System Check

2

1. Install the scan tool (tech 1) ®.
2. With the engine OFF, turn the ignition switch to the RUN position.

Important: Before clearing the DTCs, use the scan tool in order to record the Freeze Frame and Failure Records for reference. The Clear Info function will erase the data.

3. Record the DTC Freeze Frame and Failure Records.
4. Select Brake Switch on the scan tool.
5. Disconnect the brake switch connector from the brake switch.
6. Connect a test lamp from cavity D of the brake switch connector to a known good ground.

Is the test lamp ON?

--

Go to Step 3

Go to Step 4

3 | Install a fused jumper from terminal C to terminal D of the brake switch connector. Did the Brake Switch status change from Open to Closed? | -- | Go to Step 7 | Go to Step 9
4 | Remove the BRAKE fuse. Inspect the fuse for an open. Refer to Electrical Diagnosis, Section 8A. Is the fuse open? | -- | Go to Step 5 | Go to Step 8
5 | Inspect circuit 441 for a short to ground. Refer to Electrical Diagnosis, Section 8A. Did you find and correct a problem? | -- | Go to Step 11 | Go to Step 6
6 | Inspect circuit 420 for a short to ground. Refer to Electrical Diagnosis, Section 8A. Did you find and correct a problem? | -- | Go to Step 11 | Go to Step 10
7 | Replace the brake switch. Refer to Brake Switch Replacement. Is the replacement complete? | -- | Go to Step 11 | --
8 | Inspect circuit 441 for an open. Refer to Electrical Diagnosis, Section 8A. Did you find and correct a problem? | -- | Go to Step 11 | --
9 | Inspect circuit 420 for an open. Refer to Electrical Diagnosis, Section 8A. Did you find and correct a problem? | -- | Go to Step 11 | Go to Step 10
10 | Replace the VCM. Refer to VCM Replacement, Section 6. Is the replacement complete? | -- | Go to Step 11 | --

11

In order to verify your repair, perform the following procedure:

1. Select DTC.
2. Select Clear Info.
3. Ensure that the following conditions are met:

• | With the engine OFF, the ignition switch is in the RUN position.

• | The brake pedal is not depressed.

• | The Brake Switch status indicates Closed (12 volts) for 2 seconds.

4. Select Specific DTC. Enter DTC P0719.

Has the test run and passed?

--

System OK

Begin the diagnosis again. Go to Step 1