Vehicle Speed Sensor Replacement. Chevrolet Brazil Blazer 1997

For 1990-2009 cars

### Removal Procedure

#### Required Tools

J 38417 Speed Sensor Remover

1. Remove the harness connector
2. Remove the bolt.
3. Remove the vehicle speed sensor using J 38417 . Have a suitable container in order to catch the fluid.
4. Remove the O-ring seal.

### Installation Procedure

#### Required Tools

J 38417 Speed Sensor Remover

1. Install the new speed sensor and O-ring seal using J 38417 .
2. Coat the seal with a thin film of transmission fluid.
3. Install the bolt.

Tighten
Tighten the bolt to 11 N·m (97 lb in).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the harness connector.
5. Refill the fluid as required.