DTC P0502 Vehicle Speed Sensor (VSS) Circuit Low Input. Chevrolet Brazil Blazer 1997

For 1990-2009 cars
Automatic Transmission Components 4.3L
Automatic Transmission Controls Schematics 4.3L
OBD II Symbol Description Notice
Handling ESD Sensitive Parts Notice

### Circuit Description

The Vehicle Speed Sensor Assembly (VSS Assy.) provides vehicle speed information to the VCM. The VSS Assy. is a Permanent Magnet (PM) generator. The PM generator produces a pulsing AC voltage as rotor teeth on the transmission output shaft pass through the sensor's magnetic field. The AC voltage level and the number of pulses increase as the speed of the vehicle increases. The VCM then converts the pulsing voltage to vehicle speed. The VCM uses the vehicle speed signal to determine shift timing and TCC scheduling.

When the VCM detects a low vehicle speed when there is a high engine speed in a drive gear range, then DTC P0502 sets. DTC P0502 is a type A DTC.

### Conditions for Setting the DTC

• | No MAP DTC(s) P0107 or P0108.

• | No TP DTC(s) P0122 or P0123.

• | No TFP Val. Position Sw. DTC P1810.

• | The transmission is not in Park or Neutral.

• | The TP angle is greater than 20%.

• | The engine vacuum is 0-106 kPa.

• | The engine speed is greater than 3000 RPM.

• | The engine torque is 40 -400 ft lb.

• | The transmission output speed is less than 150 RPM.

• | All conditions met for 2.5 seconds.

### Action Taken When the DTC Sets

• | The VCM commands second gear only.

• | The VCM commands maximum line pressure.

• | The VCM freezes shift adapts from being updated.

• | The VCM inhibits TCC engagement.

• | The VCM illuminates the Malfunction Indicator Lamp (MIL).

### Conditions for Clearing the MIL/DTC

• | The VCM turns OFF the MIL after three consecutive ignition cycles without a failure reported.

• | A scan tool can clear the DTC from the VCM history. The VCM clears the DTC from the VCM history if the vehicle completes 40 warm-up cycles without a failure reported.

• | The VCM cancels the DTC default actions when the fault no longer exists and the ignition is OFF long enough in order to power down the VCM.

### Diagnostic Aids

• | Inspect the wiring for poor electrical connections at the VCM. Look for the following conditions:

• | A bent terminal

• | A backed out terminal

• | A damaged terminal

• | Poor terminal tension

• | A chafed wire

• | A broken wire inside the insulation

• | When diagnosing for an intermittent short or open condition, massage the wiring harness while watching the test equipment for a change.

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. This step tests the VSS Assy. circuit.

2. This step tests the integrity of the VSS Assy.

3. This step tests the 5-volt and ground circuit of the VCM.

#### DTC P0502 Vehicle Speed Sensor Assembly (VSS Assy.) Circuit -- Low Input (Transmission Output Speed Signal) (4.3L)

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Powertrain On-Board Diagnostic (OBD) System Check performed? | -- | Go to Step 2 | Go to Powertrain OBD System Check

2

1. Install the scan tool.
2. With the engine OFF, turn the ignition switch to the RUN position.

Important: Before clearing the DTCs, use the scan tool in order to record the Freeze Frame and Failure Records for reference. The Clear Info function will erase the data.

3. Record the DTC Freeze Frame and Failure Records.
4. Raise the drive wheels.
5. Start the engine.
6. Place the transmission in any drive range.

With the drive wheels rotating, does the Transmission OSS increase with the drive wheel speed?

--

Go to Diagnostic Aids

Go to Step 3

3

1. Turn the ignition OFF.
2. Disconnect the C1 (blue) VCM connector.
3. Using J 39200 DVOM and J 35616 Connector Test Adapter Kit, measure the resistance between VCM connector terminals C1-29 and C1-30.

Is the resistance within the specified range?

1470-2820 ohms

Go to Step 4

Go to Step 6

4 | Measure the resistance between terminal C1-30 and ground. Is the resistance greater than the specified value? | 50 K ohms | Go to Step 5 | Go to Step 7

5

1. Place the transmission in Neutral.
2. Select AC volts.
3. Rotate the rear wheels, ensuring that the driveshaft is turning.

Is the voltage greater than the specified value?

0.5 volts

Go to Step 8

Go to Step 9

6 | Inspect circuits 821 and 822 for an open circuit. Repair the circuits if necessary Refer to Electrical Diagnosis, Section 8A. Did you find a problem? | -- | Go to Step 15 | Go to Step 9
7 | Inspect circuits 821 and 822 for a short to ground. Repair the circuits if necessary Refer to Electrical Diagnosis, Section 8A. Did you find a problem? | -- | Go to Step 15 | Go to Diagnostic Aids

8

1. Reconnect the C1 (blue) VCM connector.
2. Disconnect the VSS Assy. harness from the VSS Assy.
3. With the engine OFF, turn the ignition switch to the RUN position.
4. Using J 39200 DVOM, measure the voltage at the VSS Assy. harness connector terminals A and B.

Is the voltage within the specified range?

4.0-5.1 volts

Go to Step 14

Go to Step 11

9

1. Remove the VSS Assy.
2. Check the output shaft speed sensor rotor for damage or misalignment.

Did you find a problem?

--

Go to Step 15

Go to Step 10

10 | Replace the VSS Assy. Refer to Vehicle Speed Sensor Assembly Replacement. Is the replacement complete? | -- | Go to Step 15 | --
11 | Was the voltage measured in Step 8 less than the voltage in the value column? | 4.0 volts | Go to Step 14 | Go to Step 12
12 | Was the voltage measured in Step 8 greater than the voltage in the value column? | 5.1 volts | Go to Step 13 | --
13 | Repair the short to B+ in circuit 821. Refer to Electrical Diagnosis, Section 8A. Is the repair complete? | -- | Go to Step 15 | --
14 | Replace the VCM. Refer to VCM Replacement, Section 6. Is the replacement complete? | -- | Go to Step 15 | --

15

In order to verify your repair, perform the following procedure:

1. Select DTC.
2. Select Clear Info.
3. Operate the vehicle, ensuring that the transmission output speed is greater than 151 RPM for 3 seconds.
4. Select Specific DTC. Enter DTC P0502.

Has the test run and passed?

--

System OK

Begin the diagnosis again. Go to Step 1