NEW PRODUCT INFORMATION PRODUCTION CHANGES 440-T4. Chevrolet Celebrity 1988

For 1990-2009 cars

# NEW PRODUCT INFORMATION PRODUCTION CHANGES 440-T4

#### Model and Year: 1988 CELEBRITY WITH THM 440-T4 TRANSAXLE

This bulletin covers New Product Information on all 1988 model THM 440-T4 transaxles. The information contained in this bulletin describes changes that occurred at the Start Of Production. Refer to each section of this bulletin for specific product change information. (Note: Figures 5 through 10 do not apply to this bulletin)

Refer to the Transaxle Hydraulic Diagnosis and Transaxle Unit Repair sections in your 1988 service manual for changes shown in this bulletin. These product changes have been identified by an asterisk (*) on the table of contents page if the change affects transaxle diagnosis, disassembly, or assembly procedures.

#### NEW MANUAL SHAFT

A new manual shaft (Figure 2, 702) that is 7mm (.276") longer is used on all 1988 THM 440-T4 transaxles. This longer manual shaft was first used on two 1987 model THM 440-T4 transaxles (7ADH, 7AHH) and is not interchangeable with the shorter manual shaft.

When servicing the subject transaxle use the proper manual shaft listed below.

Part Number Description Model Year Usage ------ ----------- ---------------- 8646946 Package, Manual Shaft and Seal 1988 - All Models (1) Shaft, Manual 1987 - 7ADH, 7AHH (1) Seal, Manual Shaft Models Only

8644923 Package, Manual Shaft and Seal 1987 - All Models (1) Shaft, Manual Except (1) Shaft, Manual Shaft 7ADH, 7AHH

This product change does not affect diagnosis, disassembly or assembly procedures for 1988 THM 440-T4 transaxles and is NOT shown in the 1988 THM 440-T4 Unit Repair Section of your service manual.

#### NEW REVERSE REACTION DRUM

A new reverse reaction drum (Figure 3, 659) is used for all 1988 subject transaxles. The change to the reverse reaction drum is identified by a chamfer on both ends of the drum.

When servicing a 1987 or 1988 THM 440-T4 the new reverse reaction drum (659) may be used. When servicing a 1984 through 1986 THM 440-T4 you must use the previous reverse reaction drum.

Part Number Description Model Year - Model Usage ------ ----------- -------------------------- 8661092 Drum, Reverse Reaction 1987-1988 - All Models

8656612 Drum, Reverse Reaction 1984-1986 - All Models

#### SERVICE MANUAL REFERENCE:

This product change does not affect diagnosis, disassembly or assembly procedures for 1988 THM 440-T4 transaxles and is not shown in the 1988 THM 440-T4 Unit Repair Section of your service manual.

#### NEW 3RD CLUTCH WAVE PLATE

A new waved 3rd clutch plate (Figure 4, 640A) instead of a flat steel plate, is used in some 1988 applications. All other 1988 model transaxles continue to use the previous design flat steel plate as part of the assembly. The new 3rd clutch plate (waved) cushions the apply of the 3rd clutch.

Transaxles models with waved 3rd clutch plate AAH, ABH, AFH, ANH, ATH, CFH, CMH, CRH, CTH, CWH, CXH. This new plate must not be used to service prior model year transaxles.

Part Number Description ------ ----------- 8656645 Plate, 3rd Clutch (waved)

#### SERVICE MANUAL REFERENCE:

This product change information is shown in the THM 440-T4 Automatic Transaxle Unit Repair section of your 1988 service manual.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.